{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"merged":[[0,0,1,7],[2,0,2,7],[3,0,3,7],[4,0,4,7],[5,0,5,7],[7,0,9,0],[7,1,9,1],[10,0,14,0],[10,1,14,1],[15,0,20,0],[15,1,20,1],[21,0,23,0],[21,1,23,1],[24,1,24,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,0,29,7],[32,2,32,6]],"flags":["formulas_cached_only"]}
["广西壮族自治区港航发展中心办公楼右侧顶层屋面漏水维修（全开挖）工程量清单"]
[]
["1、屋面总面积(电梯厅及步梯除外)：467㎡；隔热板面积198㎡；返边面积61㎡，屋面防水面积528㎡（屋面面积及返边面积）；"]
["2、工艺流程：安全文明施工围挡 → 人工翻开隔热板及支撑架 →人工打开保温层 →铲除旧防水层→基面处理→裂缝修补→刚性防水涂料1道→湿铺防水反应粘2道→"]
["沙浆找坡层→铺挤塑板→铺保护膜→铺钢网→混凝土保护层→切割伸缩缝→场地清理→竣工验收"]
[]
["序号","项目名称","分部分项工程名称","单位","数量","控制上限单价（元）","合价（元）","备 注"]
[1,"拆除部分","拆除屋面隔热板及支撑砖","㎡",198,15,null,"隔热板规格：20mx9m+7mx9m=198"]
[null,null,"拆除保温层","㎡",467,25,null,"屋面规格：24mx18m+9mx11m=467 厚度25—30cm"]
[null,null,"铲除旧防水层（屋面及返边）","㎡",528,15,null,"返边面积=(24*2+18*2+9.5/2*2)*.65=61"]
[2,"防水部分","基面打磨修补","㎡",528,50,null,"屋面及返边做防水，材料参考东方雨虹品牌"]
[null,null,"裂缝修补","m",14,95,null,"2处开裂,凿开修补，材料参考昌斯达品牌"]
[null,null,"刚性堵漏材料封堵","㎡",528,70,null,"屋面及返边做防水，材料参考昌斯达品牌"]
[null,null,"湿铺1.5厚高分子反应粘2道","㎡",528,80,null,"屋面及返边做反应粘湿铺卷材防水二遍，材料参考东方雨虹品牌"]
[null,null,"梁柱底特殊部位防水处理","根",22,165,null,"梁柱底返边做反应粘湿铺卷材防水，材料参考东方雨虹品牌"]
[3,"恢复部分","5-8CM厚C20水浆找坡","㎡",467,95]
[null,null,"铺5.0CM挤塑板","㎡",467,19]
[null,null,"铺无坊布","㎡",467,20]
[null,null,"直径6mm的钢筋网","㎡",467,15]
[null,null,"10cm厚C20水泥砂浆保护层","㎡",467,110]
[null,null,"切割伸缩缝","m",114,8,null,"5*5"]
[4,"其他","材料机械吊装费","台班",8,3000,null,"垃圾及工程材料运输"]
[null,null,"两次机械泵上浆","台班",2,4700,null,"向7楼泵送商品混凝土"]
[null,null,"垃圾清理","车",25,700,null,"10方车外运处置  运距25公里"]
["A","小计"]
["B","其他费用（施工管理费+企业利润）"]
["C"]
["D"]
["E","总计=A+B"]
["注：1.按国家相关法律法规本次补漏保修期伍年；2.以上单价不变，以实际施工量结算"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}