{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["清单"],"not_rendered":{"external_links":1,"defined_names":35},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"清单","index":0,"n_rows":13,"n_cols":9,"rows_kept":13,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["投标报价单"]
["工程名称：广西壮族自治区港航发展中心办公楼变压器采购安装工程"]
["序号","名称规格","项目特征","单位","数量","投标单价（元）","投标合价（元）","控制价上限单价\n（元）","备注"]
[1,"欧式箱变","1、箱变型号YB-12-0.4/10-630kVA;；                      2 、高压配置一面出线柜一面计量柜二面  出线柜 ；                3、 低压配置一面出线柜，一面电容柜，一面出线柜。               4、包含安装、试验","台",1,null,null,{"v":216000,"d":"216000.00"}]
[2,"箱变基础","1、箱变基础：长4800mm×宽2400mm×深1200mm；                      2 、360mm机制砖砌墙，墙面水泥砂浆抹面；                      ","座",1,null,null,{"v":8650,"d":"8650.00"}]
[3,"高压电缆","1、型号YJV22-8.5/15kV  3*70;   \n2、包含安装、试验","米",15,null,null,{"v":280,"d":"280.00"}]
[4,"高压电缆头","1、10kV NLS-3.1(冷缩电缆头）；      \n2、包含安装及试验","套",3,null,null,{"v":1400,"d":"1400.00"}]
[5,"地极角桩","热镀锌角铁∠50×5×1500","根",5,null,null,{"v":60,"d":"60.00"}]
[6,"接地扁铁","热镀锌扁铁-5*50","米",30,null,null,{"v":7.5,"d":"7.50"}]
[7,"低压进线柜","1、GGD柜宽800mm×深600mm×高2200mm;                       2、配置总进线开关1200A","面",2,null,null,{"v":28600,"d":"28600.00"}]
[9,"低压配电柜基础","1、室内配电柜基础长3200mm×宽800mm；                       2、240mm机制砖砌墙，墙面水泥砂浆抹面；                      ","项",1,null,null,{"v":8750,"d":"8750.00"}]
[10,"施工图设计","1、有资质设计单位按供电方案出具施工图纸；                         2、包含供电局图审","项",1,null,null,{"v":9450,"d":"9450.00"}]
[11,"其他费用","管理费、税金、保险等","项",1]